**DDR III 1600**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| CORSAIR | CM3X1024-1066C7 | 1GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Hynix | HMT112U6AFP8C-G7N0 | 1GB | V | V | OK |
|  | Hynix H5TQ1G83AFPG7C |  |  |  |  |
| Hynix | HMT112U6TFR8C-G7 | 1GB | V | V | OK |
|  | Hynix H5TQ1G83TFRG7C |  |  |  |  |
| Kingston | KVR1066D3N7/1G(N7K2/2G)(N7K3/3G) | 1GB | V | V | OK |
|  | Kingston D1288JPNDPLD9U |  |  |  |  |
| Samsung | M378B2873DZ1-CF8 | 1GB | V | V | OK |
|  | Samsung K4B1G0846D-HCF8 |  |  |  |  |
| Silicon Power | SP001GBLTU106S01 | 1GB | V | V | OK |
|  | Nanya NT5CB128M8AN-CG |  |  |  |  |
| Swissbit | MGU01G64D2BA1EP-BBR | 1GB | V | V | OK |
|  | Elpida J1108BASE-DJ-E |  |  |  |  |
| Swissbit | MGU12864D1BA1EP-BBR | 1GB | V | V | OK |
|  | Elpida J1108BASE-AE-E |  |  |  |  |
| TakeMS | TMS1GB364D081-107EQ | 1GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Elixir | M2F2G64CB8HA4N-BE | 2GB | V | V | OK |
|  | Elixir N2CB1G80AN-BE |  |  |  |  |
| Elixir | M2Y2G64CB8HA9N-BE | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Elixir | M2Y2G64CB8HC5N-BE | 2GB | V | V | OK |
|  | Elixir N2CB1G80CN-BE |  |  |  |  |
| Elixir | M2Y2G64CB8HC9N-BE | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Hynix | HMT125U6AFP8C-G7N0 | 2GB | V | V | OK |
|  | Hynix H5TQ1G83AFPG7C |  |  |  |  |
| Hynix | HMT125U6TFR8C-G7 | 2GB | V | V | OK |
|  | Hynix H5TQ1G83TFRG7C |  |  |  |  |
| Kingston | KVR1066D3N7/2G(N7K2/4G)(K7K3/6G) | 2GB | V | V | OK |
|  | Kingston D1288JEKAPGA7U |  |  |  |  |
| Samsung | M378B5673DZ1-CF8 | 2GB | V | V | OK |
|  | Samsung K4B1G0846D-HCF8 |  |  |  |  |
| Silicon Power | SP002GBLTU106S02 | 2GB | V | V | OK |
|  | Elixir N2CB1G80AN-BE |  |  |  |  |
| Strontium | SRT2G86U1-G7H | 2GB | V | V | OK |
|  | Hynix H5TQ1G83TFR-G7C |  |  |  |  |
| Swissbit | MGU02G64E1BA2EP-BBR | 2GB | V | V | OK |
|  | Elpida J1108BASE-AE-E |  |  |  |  |
| Swissbit | MGU02G64E2BA2EP-BBR | 2GB | V | V | OK |
|  | Elpida J1108BABG-DJ-E |  |  |  |  |
| Swissbit | MGU02G64E2BA2EP-BBR-S | 2GB | V | V | OK |
|  | Elpida J1108BASE-DJ-E |  |  |  |  |
| TakeMS | TMS2GB364D081-107EQ | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KVR1066D3N7/4G(N7K2/8G)(N7K3/12G) | 4GB | V | V | OK |
|  | Hynix H5TQ2G83AFRH9C |  |  |  |  |

**DDR III 1333**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| Apacer | 78.01GC6.9L0 | 1GB | V | V | OK |
|  | Apacer AM5D5808AEWSBG |  |  |  |  |
| G.SKILL | F3-10666CL7T-3GBPK | 1GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Hynix | HMT112U6TFR8C-H9 | 1GB | V | V | OK |
|  | Hynix H5TQ1G83TFRH9C |  |  |  |  |
| Hynix | 1GB1333D | 1GB | V | V | OK |
|  | Hynix H5TQ1G83AFRH9C |  |  |  |  |
| Hynix | CT1025 | 1GB | V | V | OK |
|  | Hynix H5TQ1283AFRH9C |  |  |  |  |
| KingMax | FLFD45F-B8KL9 [NAES] | 1GB | V | V | OK |
|  | KingMax KFB8FNLXF-BNF-15A |  |  |  |  |
| Kingston | KHX1333C9D3B1K2/2G | 1GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KVR1333D3N9/1G(N9K2/2G)(N9K3/3G) | 1GB | V | V | OK |
|  | Elpida J1108BDBG-DJ-F |  |  |  |  |
| Micron | MT4JTF12864AZ-1G4D1 | 1GB | V | V | OK |
|  | Micron D9LGQ |  |  |  |  |
| Nanya | NT1GC64B88A0NF-CG | 1GB | V | V | OK |
|  | Nanya NT5CB128M8AN-CG |  |  |  |  |
| Powerchip | AL7F8G73F-DJ2 | 1GB | V | V | OK |
|  | Powerchip A3P1GF3FGF-GDJ |  |  |  |  |
| Samsung | M378B2873FHS-CH9 | 1GB | V | V | OK |
|  | Samsung K4B1G0846F-HCH9 |  |  |  |  |
| Silicon Power | SP001GBLTU133S02 | 1GB | V | V | OK |
|  | Elixir N2CB1G80AN-CG |  |  |  |  |
| AEXEA | AXA3QS2G1333S28D | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Apacer | 78.A1GC6.9L1 | 2GB | V | V | OK |
|  | Apacer AM5D5808FEQSBG |  |  |  |  |
| Apacer | AU02GFA33C9NBGC | 2GB | V | V | OK |
|  | Apacer AM5D5808D3QSBG |  |  |  |  |
| CORSAIR | CMX8GX3M4A1333C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Crucial | BL25664BN1337.16FF | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| EasyPC | CT1037 | 2GB | V | V | OK |
|  | EasyPC CT D3 12808 |  |  |  |  |
| EKMEMORY | EKM324L28BP8-I13 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Elixir | M2F2G64CB88B7N-CG | 2GB | V | V | OK |
|  | Elixir N2CB2G80BN-CG |  |  |  |  |
| Elixir | M2F2G64CB88D7N-CG | 2GB | V | V | OK |
|  | Elixir N2CB2G80DN-CG |  |  |  |  |
| ELPIDA | 2G1333D1055A33 | 2GB | V | V | OK |
|  | ELPIDA J1108BDSE-DJ-F |  |  |  |  |
| G.SKILL | F3-10666CL7T-6GBPK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| GeIL | GG34GB1333C9DC-1.3V | 2GB | V | V | OK |
|  | GeIL GL1L128M88BA15HW |  |  |  |  |
| GOODRAM | GR1333D364L9/2G | 2GB | V | V | OK |
|  | GOODRAM GF1008KB-JN |  |  |  |  |
| GOODRAM | GR1333D364L9/2G | 2GB | V | V | OK |
|  | GOODRAM GF1008JC-JN |  |  |  |  |
| Hynix | HMT125U6TFR8C-H9 | 2GB | V | V | OK |
|  | Hynix H5TQ1G83TFRH9C |  |  |  |  |
| Hynix | HMT325U6BFR8C-H9 | 2GB | V | V | OK |
|  | Hynix H5TQ2G83BFR-H9C |  |  |  |  |
| KingMax | FLFE85F-B8KL9 [NEES] | 2GB | V | V | OK |
|  | KingMax KFB8FNLXF-BNF-15A |  |  |  |  |
| KingMax | FLFE85F-C8KM9[NAES] | 2GB | V | V | OK |
|  | KingMax KFC8FNMXF-BXX-15A |  |  |  |  |
| Kingstek | KSTD3PC-10600 | 2GB | V | V | OK |
|  | Kingstek KST3D1G1333 |  |  |  |  |
| Kingston | KHX1333C9D3B1/2G | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KVR1333D3N9/2G(N9K2/4G)(K9K3/6G) | 2GB | V | V | OK |
|  | Elpida J1108BDBG-DJ-F |  |  |  |  |
| Kingston | RBU1333D3U9DR8 | 2GB | V | V | OK |
|  | Kingston D1288JEMFPGD9U |  |  |  |  |
| KuKram | DS2G085008520013 | 2GB | V | V | OK |
|  | KuKram SADU25680-D1333 |  |  |  |  |
| Micron | MT8JTF25664AZ-1G4D1 | 2GB | V | V | OK |
|  | Micron D9LCK |  |  |  |  |
| Nanya | NT2GC64B8HA0NF-CG | 2GB | V | V | OK |
|  | Nanya NT5CB128M8AN-CG |  |  |  |  |
| OCZ | OCZ3G1333LV4GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PSD32G13332 | 2GB | V | V | OK |
|  | Patriot PM128M8D3BU-15 |  |  |  |  |
| Powerchip | AL8F8G73F-DJ2 | 2GB | V | V | OK |
|  | Powerchip A3P1GF3FGF-GDJ |  |  |  |  |
| Samsung | M378B5673FH0-CH9 | 2GB | V | V | OK |
|  | Samsung K4B1G0846F-HCH9 |  |  |  |  |
| Samsung | M378B5773DH0-CH9 | 2GB | V | V | OK |
|  | Samsung K4B2G0846D-HCH9 |  |  |  |  |
| SanMax | SMD-2G88H1P-13HZ | 2GB | V | V | OK |
|  | Hynix H5TQ1G83BFRH9C |  |  |  |  |
| SanMax | SMD-2G88N7P-13HM | 2GB | V | V | OK |
|  | Elpida J1108BFBG-DJ-F |  |  |  |  |
| SanMax | SMD-2G88N7VLP-13HM | 2GB | V | V | OK |
|  | Elpida J1108BFSE-DJ-F |  |  |  |  |
| Silicon Power | SP002GBLTU133S02 | 2GB | V | V | OK |
|  | Elixir N2CB1G80AN-CG |  |  |  |  |
| Spectek | 122010-W10 | 2GB | V | V | OK |
|  | Spectek 128X8DDR3 |  |  |  |  |
| Spider | H200UD12808-1333A | 2GB | V | V | OK |
|  | Spider H1081333EE1105G |  |  |  |  |
| Strontium | SRT2G86U1-H9H | 2GB | V | V | OK |
|  | Hynix H5TQ1G83TFR-H9C |  |  |  |  |
| UMAX | E41302GP0-73BDB | 2GB | V | V | OK |
|  | UMAX U2S24D30TP-13 |  |  |  |  |
| Winchip | GDF2GB18L150C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Apacer | 78.B1GDE.9L10C | 4GB | V | V | OK |
|  | Apacer AM5D5908CEHSBG |  |  |  |  |
| Elixir | M2F4G64CB8HB5N-CG | 4GB | V | V | OK |
|  | Elixir N2CB2G80BN-CG |  |  |  |  |
| Elixir | M2F4G64CB8HD5N-CG | 4GB | V | V | OK |
|  | Elixir N2CB2G80DN-CG |  |  |  |  |
| G.SKILL | F3-10666CL7D-8GBRH | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-10666CL9D-8GBRL | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Hynix | HMT351U6AFR8C-H9 | 4GB | V | V | OK |
|  | Hynix H5TQ2G83AFRH9C |  |  |  |  |
| Hynix | HMT351U6BFR8C-H9 | 4GB | V | V | OK |
|  | Hynix H5TQ2G83BFR-H9C |  |  |  |  |
| KingMax | FLFF65F-C8KM9[NEES] | 4GB | V | V | OK |
|  | KingMax KFC8FNMXF-BXX-15A |  |  |  |  |
| Kingston | KVR1333D3N9/4G(N9K2/8G)(N9K3/12G) | 4GB | V | V | OK |
|  | Hynix H5TQ2G83AFRH9C |  |  |  |  |
| Micron | MT16JTF51264AZ-1G4D1 | 4GB | V | V | OK |
|  | Micron D9LGK |  |  |  |  |
| Samsung | M378B5273CH0-CH9 | 4GB | V | V | OK |
|  | Samsung K4B2G0846C-HCH9 |  |  |  |  |
| Samsung | M378B5273DH0-CH9 | 4GB | V | V | OK |
|  | Samsung K4B2G0846D-HCH9 |  |  |  |  |
| Strontium | SRT4G86U1-H9H | 4GB | V | V | OK |
|  | Hynix H5TQ2G83MFR-H9C |  |  |  |  |

**DDR III 1333 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| A-DATA | AXDU1333GC2G9-2G | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1333C7D3K3/6GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1333C7D3K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1333C9D3K2/4G | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1333C9D3UK2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 1500 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| GeIL | GEP34GB1500C9DC | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 1600 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| CORSAIR | CMZ6GX3M3A1600C8 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMZ6GX3M3A1600C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| EKMEMORY | EKM324L28BP8-I16 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL7D-4GBRM | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| GeIL | GB34GB1600C8DC | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| KingMax | FLGE85F-C8KJ9A FAIS | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C7D3K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9AD3/2G | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3B1K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3K3/6GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3LK2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3T1BK3/12GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3T1BK3/6GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3T1K3/6GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3X2K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| OCZ | OCZ3BE1600C8LV4GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| OCZ | OCZ3X1600R2LV6GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PG234G1600ELKA | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PG234G1600LLKA | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PGS34G1600LLKA2 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PVV34G1600LLK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PXD34G1600LLK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Princo | TB1600CL7D3-2GB | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Strontium | SRG2G88U2-P9H | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| TakeMS | TMS2GB364D081-169KN | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Winchip | GDF2GB18L125C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| WINTEC | 3OH16009U9H-4GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| WINTEC | 3OH16009U9H-6GT | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Elixir | M2Y2G64CB8HA9N-DG | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KVR1600D3N11/2G-ES | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| A-DATA | AX3U1600GC4G9-DG2 | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| A-DATA | AX3U1600XC4G79-2X | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMZ8GX3M2A1600C9 | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL7D-8GBRH | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL8D-8GBECO | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL9D-8GBRL | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PG238G1600ELKA | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PGD38G1600ELK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PX538G1600LLK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PX7312G1600LLK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PXD38G1600LLK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| WINTEC | 3OH16009U9H-12GT | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| WINTEC | 3OH16009U9H-8GK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL7D-8GBXH | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL9D-8GBSR2 | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-12800CL9Q-16GBXL | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX1600C9D3P1K2/8G | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PSD38G1600KH | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 1750 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| GeIL | GEP34GB1750C9DC | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 1800 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| Patriot | PVV34G1800LLK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 1866 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| OCZ | OCZ3RPR1866C9LV6GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMT6GX3M3A1866C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMT12GX3M6A1866C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMT8GX3M4A1866C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Princo | TB1866CL8D3-2GB | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PXD34G1866ELK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-14900CL9D-8GBSR | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-14900CL9Q-16GBXL | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PXD38G1866ELK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 2000 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| A-DATA | AX3U2000GB2G9B-2G | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMG4GX3M2A2000C8 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMT6GX3M3A2000C8 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMX4GX3M2A2000C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMX6GX3M3A2000C9 | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| EXCELERAM | E30119A | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-16000CL7D-4GBFLS | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| G.SKILL | F3-16000CL9T-6GBTD | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX2000C9AD3T1K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX2000C9AD3W1K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX2000C9AD3W1K3/6GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| OCZ | OCZ3RPR2000LV4GK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PGV34G2000ELK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PX534G2000ELK | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Strontium | SRG2G88U3-V9H | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| A-DATA | AX3U2000GC4G9B-DG2 | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| CORSAIR | CMX12GX3M3A2000C9 | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Patriot | PX7312G2000ELK | 4GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 2133 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| Kingston | KHX2133C9AD3T1K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |
| Kingston | KHX2133C9AD3W1K2/4GX | 2GB | V | V | OK |
|  | 鐵殼 |  |  |  |  |

**DDR III 2333 OC**

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | **Model** | **Size** | **2 DIMMs** | **4 DIMMs** | **R.S.T** |
| Kingston | KHX2333C9D3T1K2/4GX | 2GB | V |  | OK |
|  | 鐵殼 |  |  |  |  |